### Bibby Pioneer

### Multi-purpose barge



### General Information

|  |  |
| --- | --- |
| Type of Barge: | +A1, Barge + Notation ‘Accommodation Barge’ |
| Port of Registry: | Bridgetown |
| Classification: | American Bureau of Shipping (ABS) |
| Built: | 2007, Nantong Tongcheng Ship Manufacturing Co. Ltd., modified 2010/11 in Glasgow UK |
| Length: | 100.6 metres |
| Breadth: | 30.48 metres |
| Depth: | 6.09 metres |
| Gross Tonnage: | 7599 tonnes |
| Net Tonnage: | 2279 tonnes |
| Deck Capacity: | 15 tonnes/m² |
| Free Deck Area: | 1,100m² |
| Fresh Water Capacity: | 1,360 m³ |
| Fuel Oil: | 613 m³ |
| Load Line: | International Load Line certificate issued by ABS |
| Main Generators: | 3 x 900 kW at 440 v 60 Hz 3 ph |
| Emergency Generator: | 1 x 900 kW at 440 v 60 Hz 3 ph |
| Mezz Deck Service Crane:  | 7.5 tonnes at 25 metres maximum lifting capacity |
| Mooring: | 8 point mooring system, 4 x 100 tonne double drum winches equipped with 1100 metres x 58 mm wire, tension monitoring system and local and remote control facilities. 4 x 12 tonne primary anchors & 4 x 7 tonne secondary anchors |
| Gangway: | 2 position gangway port side |
| Boat Landings: | Port and stbd for CTV transfers |
| Rescue Boat: | Davit Launch rescue boat – Port side |
| Galley: | Fully equipped, state of the art, galley and mess room |
| Accommodation: | Serviced accommodation for up to 120 POB (upgradeable to 240 POB) |